**TREE VISUAL CONDITION CHECKLIST**

* The *Tree Visual Condition Checklist: Guidance* document should be used to facilitate the visual inspection.
* Any defects should be recorded in the table below.
* Trees should be visually inspected from ground level.
* It is sufficient initially to look for external signs that may indicate a hazard exists. If no significant hazard revealed, further action is not generally required until next inspection.
* If evidence of a hazard is found, more detailed investigation by a specialist is recommended
* Only a qualified, trained specialist should undertake remedial works on trees.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date** | **Tree ID / Location** | **Signature** | **Observation / Actions** | **Remedial Work Complete** |
| **Date** | **Sign** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |